Device Register Information:
Status Register:
  Bit        Name                            Settings:    
   7         Status Register Write Enable    0: Enabled(Default), 1: Disabled
  5-2        BP[3:0]                         See Protected Area table