Register definition: 
Status Register 1: S7 - S0
  Bit        Name                              Settings:    
   7         Status Register Protect 0         0: Disabled(Default), 1: Enabled
  6-2        Block Protection Bits[4:0]        See Protected Area table

Status Register 2: S15 - S8
  Bit        Name                              Settings:    
   6         Complement Protect                0: Non-Reversed, 1: Reversed
  5-3        Security Register Lock Bits 3-1   0: Unlocked(Default) 1: Locked (OTP)
   1         Quad Enable                       0: Disabled, 1: Enabled
   0         Status Register Protect 1         Volatile Protection bit

Status Register 3: S23 - S16
  Bit        Name                              Settings:
  6-5       DRV 1-0                           See Driver Encoding table