Device Register Information:
Status Register:
  Bit        Name                            Settings:    
   7         Status Register Write Enable    0: Enabled (Default), 1: Disabled
   6         QE - Quad Bit                   0: Disabled (Default), 1: Enabled
  5-2        BP[3:0]                         See Protected Area table

Security Register:
  Bit        Name                            Settings:    
   1         LDSO (Lock Down Security OTP)   0: Disabled (Default), 1: Enabled