Register definition: 
Status Register 1: S7 - S0
  Bit		Name                                Settings
   7		Status Register Protection 0        0: Disabled (Default), 1: Enabled
  6-2		Block Protect Bits[4:0]             See Protected Area Table

Status Register 2: S15 - S8
  Bit		Name                                Settings
  14		Complement Protect Bit              0: Disabled (Default), 1: Enabled
  12		Dummy Configuration Bit             0: 4 or 6 Dummy Cycles, 1: 8 or 10 Dummy Cycles
  11		Security Register Lock Bit 1        0: Unlocked, 1: Locked (OTP)
  10		Security Register Lock Bit 0        0: Unlocked, 1: Locked (OTP)
   9		Quad Enable                         1: Enabled Permanently