Register definition: 
Status Register 1: S7 - S0
  Bit		Name                                Settings
   7		Status Register Protection 0        0: Disabled (Default), 1: Enabled
  6-2		Block Protect Bits[4:0]             See Protected Area Table

Status Register 2: S15 - S8
  Bit		Name                                Settings
  11		Security Register Lock Bit          0: Unlocked, 1: Locked (OTP)
   9		Reserved as 1

Configuration Register Byte 1: 7 - 0
  Bit		Name                                Settings
  4-0		Dummy Cycle Configuration           Default: 6 (0x06)

Minimum value for dummy cycle configuration is 3 (0x03), maximum value is 30 (0x1E)

Configuration Register Byte 3: 7 - 0
  Bit		Name                                Settings
  7-4		On Die Termination                  Default: ODT Disabled (0b1111xxxx)
  3-0		Driver Strength Configuration       Default: 50 Ohm (0xFF)

Configuration Register Byte 4: 7 - 0
  Bit		Name                                Settings	
   3		DLP Configuration                   Default: DLP Disabled (0bxxxx1xxx)
   2		Protection Configuration            Default: BP Protection (0bxxxxx1xx)

Configuration Register Byte 5: 7 - 0
  Bit		Name                                Settings
   0		Beyond 128Mb Address Configuration  0: Enabled, 1: Disabled (Default)

Configuration Register Byte 6: 7 - 0
  Bit		Name                                Settings
   0		XIP Configuration                   0: Enabled, 1: Disabled (Default)

Configuration Register byte 7: 7 - 0
  Bit		Name                                Settings
  1-0		Wrap Configuration                  11: Wrap Disabled (Default), 10: 64-Byte Wrap, 01: 32-Byte Wrap, 00: 16-Byte Wrap