This Algorithm support 2 Flash Banks:
Byte Address    WORD Address    Notes
  0x100000        0x80000       Flash Bank 0
  0x120000        0x90000       Flash Bank 1
                

User configurable DCSM OTP Banks are not yet supported.